{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["Sheet1","2023年使用量"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":8,"n_cols":9,"rows_kept":8,"merged":[[7,1,7,8]]}
["序号","名称","参考规格","项目概况","技术参数","参考品牌","预计使用量","限价","使用科室"]
[1,"二氧化锆","全瓷冠、桥",null,"材料强度800-1100MPa",null,10,500,"口腔科"]
[2,"钛支架","钛合金激光烧结支架可摘局部义齿",null,"切削支架的连接体和卡环无气孔，裂纹和杂质，卡环体与卡环臂连接处的厚度不小于1.0mm，前腭杆厚度大于等于1.0mm,后腭杆厚度为1.2-2.0mm.腭板的厚度不小于0.5 mm。",null,5,800,"口腔科"]
[3,"普通牙","树脂基托局部义齿",null,"人工牙的功能尖位于牙槽嵴顶",null,60,22,"口腔科"]
[4,"正畸矫治器","激光选区熔化钴铬合金支架型固定矫治器",null,"边缘光滑，矫治器的树脂基托部分最薄处应不小于0.6mm",null,2,750,"口腔科"]
[5,"正畸矫治器","固定矫治器",null,"边缘光滑，矫治器的树脂基托部分最薄处应不小于0.6mm",null,6,300,"口腔科"]
[6,"正畸矫治器","树脂基托式扩弓矫治器",null,"边缘光滑，矫治器的树脂基托部分最薄处应不小于0.6mm",null,5,700,"口腔科"]
["备注","售后服务要求：1.所投产品符合国家相关质量标准及采购人验收要求。\n2.提供全年原厂7*24小时技术支持（提供承诺函）。\n3.供应及时，响应迅速，不影响医院正常医疗秩序。\n4.验收或使用过程中如发现存在质量问题，应及时派人到现场行进退换货处理，由此产生的一切责任与费用由投标人承担（提供承诺函）。\n5.供货过程中如存在虚假、欺骗等行为，采购人有权对投标人处罚违约金。情节严重的招标人有权提前终止合同，甚至交政府相关部门处置（提供承诺函）。\n6.如产品带量采购则按照带量采购文件执行（提供承诺函）。\n7.为保持产品一致性，所投产品需为同一生产厂家生产的产品。"]

{"sheet":"2023年使用量","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}